# Smart Factory Enterprise Synchronization Workflow
*Optimized for AI-Tadpole-OS*

## Objective
To maintain a high-frequency, low-latency synchronization between the physical factory floor and the enterprise ERP/Digital Twin systems.

## Steps
1. **Design Sync**: `R&D Liaison` monitors PLM/CAD folders for new engineering releases and translates them into production specs.
2. **Virtual Commissioning**: `Digital Twin Sync` simulates the impact of the new design on the current production line using the digital twin model.
3. **Enterprise Approval**: Once simulation passes, the `ERPSync Master` pushes the updated bill of materials (BOM) to the central ERP (SAP/Oracle).
4. **Execution**:
   - The shop floor agents (see 25/50 seat templates) execute the production run.
   - Real-time performance data is fed back into the `Digital Twin Sync`.
5. **Continuous Optimization**: The `ERPSync Master` identifies variances between the ERP's "Planned Cost" and the actual swarm "Live Cost" to optimize future budgets.

## Compliance & Governance
- Every design-to-production transfer is logged on the Merkle Audit Trail.
- Any change to the BOM requires a multi-agent consensus (Oversight Gate).
