# Workflow: Cold-Chain Inbound Release SOP

## Step 1

Retrieve temperature tracking USB sensor from the shipping box.
## Step 2

Check temperature history to ensure no cold-chain breaks occurred.
## Step 3

Output GMP conformity release and transfer products to warehouse freezers.
