Skip to content

Pocket synthesizer · Norm Audio

# FIELD-7

Sixteen pads, two knobs, and an engine that fits in a jacket pocket without asking permission.

$329 USD · shipping calculated later

Buy FIELD-7
DWG · TOP VIEW SCALE 1:2 · REV C

### Dimensions

W
  148.0 mm
D
  88.0 mm
H
  28.0 mm
Mass
  312 g

01 · Callouts

## Pinned to the drawing

A

### Pad matrix

Sixteen velocity-sensitive pads in a 4 by 4 grid. Soft enough for thumbs, firm enough that you stop blaming the firmware.

B

### Dual knobs

Filter and level. Aluminum, detented just enough. No third knob for “vibe.”

C

### OLED strip

Patch name, BPM, battery. Monochrome on purpose. It is a meter, not a billboard.

D

### Speaker grille

Front-facing driver for desk checks. Quiet rooms will still notice. Headphones remain the adult option.

02 · In the box

## Knolled kit

USB-C cable1.2 m
Soft caseGray
Neck strapAdjustable
Battery packSpare

03 · Specification

## Engineering sheet

Model | FIELD-7 pocket synthesizer
Maker | Norm Audio (fictional)
Dimensions (W × D × H) | 148.0 × 88.0 × 28.0 mm
Weight | 312 g (with battery)
Battery | 3.7 V 2200 mAh Li-ion · ~8 h typical play · USB-C charge
I/O | USB-C (MIDI + power) · 3.5 mm stereo out · 3.5 mm sync I/O
Controls | 16 velocity pads · 2 continuous knobs · power switch
Display | 128 × 32 monochrome OLED
Sound engines | 4 oscillators · 2 LFOs · 1 multimode filter · 8-voice polyphony
Sequencer | 64-step · 8 patterns · probability per step
Speaker | 28 mm full-range · front grille
Finish | Matte panel gray · orange index marks

## Order FIELD-7

Visual checkout only on this demo page. Price holds at $329 USD. Ships in a recycled pulp tray; no mystery foam peanuts.

Read specs

Demo control — no payment is collected.

Shipping: 5–9 business days within the continental fiction zone.
Warranty: 24 months parts and labor against manufacturing defects. Pads worn through from honest use are not defects — they are a resume.
Returns: 30 days, device and kit complete, no sticky labels on the OLED.